(footprint "ResetBtn"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(hide yes)
		(uuid "f04ab01c-8438-47ff-87f1-f356246c0a08")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "ResetBtn"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8c3f3ec1-cbe4-4b14-ad20-984bf42c07bb")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2c3f77e5-b81e-466f-9013-c63d66283bb1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "36049c07-b402-4b32-b981-88ced9c526a4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -3 -3)
		(end 3 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "80d65b0b-efe3-4b83-841b-5350934369bd")
	)
	(fp_rect
		(start -3 -3)
		(end 3 3)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "B.SilkS")
		(uuid "1874c6fe-dbe7-4cf0-91f0-4d59ce3dc561")
	)
	(fp_circle
		(center 0 0)
		(end 2 -1.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "062f7d7d-34f8-498e-9266-e6a02e903bb4")
	)
	(pad "1" smd roundrect
		(at -3 -3)
		(size 3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "4f9410ee-2327-456c-a446-ecba82ee68b7")
	)
	(pad "1" smd roundrect
		(at -3 -3)
		(size 3 3)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "734989d2-5cf5-4442-bb97-40b8a71b1054")
	)
	(pad "1" smd roundrect
		(at 3 -3)
		(size 3 3)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "71e3e2e2-c285-430c-b5ba-094d48616b40")
	)
	(pad "2" smd roundrect
		(at 3 -3)
		(size 3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "645d6d56-b756-4bc0-860f-c017b026effd")
	)
	(pad "3" smd roundrect
		(at 3 3)
		(size 3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "945583b9-939d-4dc5-bcd0-0283f9c67254")
	)
	(pad "3" smd roundrect
		(at 3 3)
		(size 3 3)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "1de70a3e-cd63-4633-b073-b081bb57f412")
	)
	(pad "4" smd roundrect
		(at -3 3)
		(size 3 3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "8e0045d6-5f14-4700-92eb-34bc4f815967")
	)
	(pad "4" smd roundrect
		(at -3 3)
		(size 3 3)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.15)
		(thermal_bridge_angle 45)
		(uuid "2213f376-41ae-4f29-92a4-75fa708d656d")
	)
	(embedded_fonts no)
)
