(footprint "MOUDLE14P-XIAO-HALF-HOLE-PRO"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0.0523 -10.696 0)
		(unlocked yes)
		(layer "User.4")
		(uuid "9c00e526-d413-475c-bc1e-35e31ee7f907")
		(effects
			(font (size 0.2032 0.254) (thickness 0.0508))
		)
	)
	(property "Value" "XIAO Pin"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "d0c221fd-2e1c-49b0-91c2-be5348d225f3")
		(effects
			(font (size 0.635 0.635) (thickness 0.1016))
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "54725d32-0ed3-4666-b6ab-8591e736d541")
		(effects
			(font (size 1.27 1.27) (thickness 0.15))
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2cd1e500-fe6f-4419-a630-fc76d21a4235")
		(effects
			(font (size 1.27 1.27) (thickness 0.15))
		)
	)
	(property "MPN" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "605c0f7d-9c15-4a04-b8b0-6450e8768a99")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "Manufacturer" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "e47dfc3f-46a7-4cb4-823c-8eb4e1d6afbc")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "Part Type" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "b2601143-fc2d-4286-a30a-bedb5c1cfc1b")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "Rating" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2387cebb-15df-4967-bfd8-44df075cd18b")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "SKU" "XIAO-HALF-HOLE"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d4fac908-1a3c-4035-b4ec-0d811dafab1b")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "Status" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "155f282b-51d2-485b-a5f1-473b5ce37e38")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "Temperature" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "2832cfd3-55d2-45e4-a11a-ef632ab9562e")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(property "Priority" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ac204f07-9463-4b0e-b9ee-7c0a79ffdcc9")
		(effects
			(font (size 1 1) (thickness 0.15))
		)
	)
	(attr smd)
	(net_tie_pad_groups "1" "2" "3" "4" "5" "6" "7" "8" "9" "10" "11" "12" "13"
		"14"
	)
	(fp_line
		(start -10.414 -6.985)
		(end -10.414 6.985)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "124df625-be58-4b39-bf4b-9e7cfe109aac")
	)
	(fp_line
		(start -8.509 -8.89)
		(end 8.636 -8.89)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "5a1509dd-81a4-49ea-9cf8-bba067cb1dcc")
	)
	(fp_line
		(start -8.509 8.89)
		(end 8.636 8.89)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "ac7e97e0-bfd7-4431-9c8c-4b15ffc5b3a9")
	)
	(fp_line
		(start 10.541 6.985)
		(end 10.541 -6.985)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "0a8696a8-122f-4a65-8052-0846988966a4")
	)
	(fp_arc
		(start -10.414 -6.985)
		(mid -9.856038 -8.332038)
		(end -8.509 -8.89)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "d998c230-c2c1-41ba-be1b-12cb69347786")
	)
	(fp_arc
		(start -8.509 8.89)
		(mid -9.856038 8.332038)
		(end -10.414 6.985)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "3185e033-c137-4132-b13f-bdf3021208b8")
	)
	(fp_arc
		(start 8.636 -8.89)
		(mid 9.983038 -8.332038)
		(end 10.541 -6.985)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "5f1aa4ea-8f5c-4189-9f50-b173af13eeaf")
	)
	(fp_arc
		(start 10.541 6.985)
		(mid 9.983038 8.332038)
		(end 8.636 8.89)
		(stroke (width 0.0254) (type solid))
		(layer "Edge.Cuts")
		(uuid "8547de4c-7895-46ed-9ff8-c499c542c317")
	)
	(fp_line
		(start 10.57 4.5161)
		(end 10.57 -4.485)
		(stroke (width 0.1) (type default))
		(layer "User.1")
		(uuid "4bd5d798-9102-4133-8478-572ac571ebfc")
	)
	(fp_line
		(start 10.58 -4.485)
		(end 12.0819 -4.485)
		(stroke (width 0.1) (type default))
		(layer "User.1")
		(uuid "7337be9b-2040-479d-a0f8-9d3a743fec1f")
	)
	(fp_line
		(start 12.0819 -4.485)
		(end 12.0819 4.5161)
		(stroke (width 0.1) (type default))
		(layer "User.1")
		(uuid "c2a92c8e-0c1f-443d-8c18-88de2228a960")
	)
	(fp_line
		(start 12.0819 4.5161)
		(end 10.57 4.5161)
		(stroke (width 0.1) (type default))
		(layer "User.1")
		(uuid "0b0e22c2-cdc7-4999-857e-4fecdd36ba90")
	)
	(fp_rect
		(start 5.715 -3.81)
		(end 12.065 3.81)
		(stroke (width 0.0762) (type default))
		(fill no)
		(layer "User.1")
		(uuid "a11626c3-151d-495a-bb0e-a4b701007f80")
	)
	(fp_circle
		(center -7.62 -7.62)
		(end -7.493 -7.62)
		(stroke (width 0.0254) (type default))
		(fill no)
		(layer "User.1")
		(uuid "5bda0957-545a-46f5-85e7-65c8738846db")
	)
	(fp_circle
		(center 7.62 7.62)
		(end 7.493 7.62)
		(stroke (width 0.0254) (type default))
		(fill no)
		(layer "User.1")
		(uuid "2186e2c7-7c94-4959-b312-e871f2c3e1e4")
	)
	(pad "1" thru_hole circle
		(at 7.62 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "2a582eeb-3337-49f1-aef9-1c9ce213726e")
	)
	(pad "1" smd roundrect
		(at 7.62 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "1c55721a-392c-4254-82c5-e929ecd6faa9")
	)
	(pad "1" smd roundrect
		(at 7.62 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "eb2c2c17-94fa-424d-b0b3-01027ac7e7de")
	)
	(pad "1" thru_hole circle
		(at 7.62 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "86892b3b-f244-40cb-abf7-19218aff54ab")
	)
	(pad "2" thru_hole circle
		(at 5.08 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "8656bc28-993a-450f-9f46-b5ea0551ddbd")
	)
	(pad "2" smd roundrect
		(at 5.08 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "704ee6cc-e810-49ab-9290-925a320a6d81")
	)
	(pad "2" smd roundrect
		(at 5.08 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "f9746368-1452-4a2b-b715-2c08aaa7a8f0")
	)
	(pad "2" thru_hole circle
		(at 5.08 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "86b9a616-89b9-4792-a961-3a73db4aee4d")
	)
	(pad "3" thru_hole circle
		(at 2.54 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "5ceb9237-75b1-4a1a-98ef-ae7b71abc752")
	)
	(pad "3" smd roundrect
		(at 2.54 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "4e298f86-15ef-4963-aab1-1270ef47e597")
	)
	(pad "3" smd roundrect
		(at 2.54 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "923f549d-a9d2-4948-b9d9-96bd890774b4")
	)
	(pad "3" thru_hole circle
		(at 2.54 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "78d5ce6e-0ef8-44dc-a8cd-af6518eaaf54")
	)
	(pad "4" thru_hole circle
		(at 0 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "304cdfb9-0861-4f1f-be54-1b996d9d6789")
	)
	(pad "4" smd roundrect
		(at 0 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "d33b466c-e782-4025-abc6-2114b12dc64c")
	)
	(pad "4" smd roundrect
		(at 0 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "b9fc4f0a-e242-41c3-8c02-63c7b50b643c")
	)
	(pad "4" thru_hole circle
		(at 0 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "a27220bf-d179-4464-9294-994b67cd023b")
	)
	(pad "5" thru_hole circle
		(at -2.54 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "e01146f7-f062-4644-a064-ebcf4a9a1412")
	)
	(pad "5" smd roundrect
		(at -2.54 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "0c5b8fa8-3589-44d2-a65e-79afea54068c")
	)
	(pad "5" smd roundrect
		(at -2.54 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "ce4befb7-02df-456b-a1d0-ef4240e28928")
	)
	(pad "5" thru_hole circle
		(at -2.54 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "8858cf7d-1d74-40aa-bccb-9e0acf75c690")
	)
	(pad "6" thru_hole circle
		(at -5.08 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "ff367f8b-85ac-44c0-9912-f99d2fd8b5a1")
	)
	(pad "6" smd roundrect
		(at -5.08 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "e6adadf7-7fca-430f-b1d7-70bdc0d80962")
	)
	(pad "6" smd roundrect
		(at -5.08 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "05efdfcd-3e51-4282-9c73-ea9607acfb63")
	)
	(pad "6" thru_hole circle
		(at -5.08 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "ac8d78ea-4541-4799-8960-75fb149ca69e")
	)
	(pad "7" thru_hole circle
		(at -7.62 -8.89 180)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "53195c04-cebe-4197-8570-7e2e0f426820")
	)
	(pad "7" smd roundrect
		(at -7.62 -8.028)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "6586792a-d576-41c6-9cc7-d44d690596a2")
	)
	(pad "7" smd roundrect
		(at -7.62 -8.028)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "eb697a12-4aea-4cf6-b1a7-60de205b10d3")
	)
	(pad "7" thru_hole circle
		(at -7.62 -7.62 270)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "0e615fa8-73ce-481b-a1f1-fb662a1ff429")
	)
	(pad "8" thru_hole circle
		(at -7.62 7.62 270)
		(size 0.95 0.95)
		(drill 0.889)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "87deb5f9-b71f-4651-9929-7a2b4489a470")
	)
	(pad "8" smd roundrect
		(at -7.62 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "e21c2b9c-473d-4843-b528-083ae4bbba02")
	)
	(pad "8" smd roundrect
		(at -7.62 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "058e6e2e-b073-42ae-a6ae-8ed7afdd812c")
	)
	(pad "8" thru_hole circle
		(at -7.62 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "d7ce3a08-913b-496b-8a4c-7bc4bcc31c49")
	)
	(pad "9" thru_hole circle
		(at -5.08 7.62 90)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "e3cd7296-d105-4816-bc08-f44f172d5405")
	)
	(pad "9" smd roundrect
		(at -5.08 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "2c3f3fe4-64f0-400f-8cdf-5079c25fb3f3")
	)
	(pad "9" smd roundrect
		(at -5.08 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "7a242e9f-ac0e-45f7-aabb-8a5aa7e5ec90")
	)
	(pad "9" thru_hole circle
		(at -5.08 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "c7642ba1-02a0-4a1d-b51f-1726eac2b536")
	)
	(pad "10" thru_hole circle
		(at -2.54 7.62 90)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "54c31d57-7a1e-4ba1-893f-fb0bb946be92")
	)
	(pad "10" smd roundrect
		(at -2.54 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "f32af148-742d-4e77-b98b-17ae3a506252")
	)
	(pad "10" smd roundrect
		(at -2.54 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "3d5fbf6e-de52-4d28-9142-10643b9c885b")
	)
	(pad "10" thru_hole circle
		(at -2.54 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "90279435-19ef-4a9d-afc0-ce80d8e41a9e")
	)
	(pad "11" thru_hole circle
		(at 0 7.62 90)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "e69bbb7d-46a2-4f9f-9e18-b2b5ea3833ba")
	)
	(pad "11" smd roundrect
		(at 0 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "e224370e-91b9-4e1a-9a85-9b9781785873")
	)
	(pad "11" smd roundrect
		(at 0 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "ae3f2035-988e-442b-964d-6b4f87056376")
	)
	(pad "11" thru_hole circle
		(at 0 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "b2a7e68f-3d75-428f-8520-f46bb9f3ee05")
	)
	(pad "12" thru_hole circle
		(at 2.54 7.62 90)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "3d266da4-5a2d-4126-8aa4-e321746521f8")
	)
	(pad "12" smd roundrect
		(at 2.54 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "ba3029e8-1bb7-4515-99c6-b49cba20718c")
	)
	(pad "12" smd roundrect
		(at 2.54 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "c6670a4a-53b4-4ad5-a628-007ef1f631d0")
	)
	(pad "12" thru_hole circle
		(at 2.54 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "27390810-3cff-4b96-bd10-cf87f15afc39")
	)
	(pad "13" thru_hole circle
		(at 5.08 7.62 90)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "021403d6-7f82-47b3-a622-1d0933ac6c5f")
	)
	(pad "13" smd roundrect
		(at 5.08 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "cdc30211-61de-4fda-9a96-b31c9230e38d")
	)
	(pad "13" smd roundrect
		(at 5.08 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "8b1d3d30-e692-444b-8b25-11509bd41573")
	)
	(pad "13" thru_hole circle
		(at 5.08 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "3c57c0bd-6320-4c07-8046-e47844e4768f")
	)
	(pad "14" thru_hole circle
		(at 7.62 7.62 90)
		(size 0.95 0.95)
		(drill 0.85)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "64094c5b-7495-4578-a920-9c5a642c18f3")
	)
	(pad "14" smd roundrect
		(at 7.62 8.028 180)
		(size 1.626 1.725)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0.01)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "8e466c24-9227-4465-8fc7-d38356c715b0")
	)
	(pad "14" smd roundrect
		(at 7.62 8.028 180)
		(size 1.626 1.725)
		(layers "B.Cu" "B.Mask" "B.Paste")
		(roundrect_rratio 0.5)
		(chamfer_ratio 0)
		(chamfer top_left top_right)
		(solder_mask_margin 0.05)
		(uuid "3bc19e5d-c3b9-4f68-8b2d-a5ae294cf29a")
	)
	(pad "14" thru_hole circle
		(at 7.62 8.89)
		(size 1.27 1.27)
		(drill 0.7)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0.0254)
		(uuid "5feba75e-151e-46a6-9c67-3ac610762c9a")
	)
	(embedded_fonts no)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-nRF52840 v15.step"
		(hide yes)
		(offset (xyz -1.778 -6.096 0.381))
		(scale (xyz 1 1 1))
		(rotate (xyz -90 0 0))
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeeduino XIAO SAMD21 v4.step"
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 0))
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO RP2040 v26.step"
		(hide yes)
		(offset (xyz 0 0 0))
		(scale (xyz 1 1 1))
		(rotate (xyz 0 0 90))
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/Seeed Studio XIAO-ESP32-C3.step"
		(hide yes)
		(offset (xyz -1.7018 -6.096 0))
		(scale (xyz 1 1 1))
		(rotate (xyz -90 0 0))
	)
	(model "${AMZPATH}/3dmodels/AMz3D.3dshapes/XIAO-ESP32S3 v2.step"
		(hide yes)
		(offset (xyz -1.778 -6.1722 0))
		(scale (xyz 1 1 1))
		(rotate (xyz -90 0 0))
	)
)
